## Using on board Red, Green and Blue led (GPIO)