## Using IO Expander to drive LEDs (non-interrupt driven) (I2C)