## Interfacing external temperature sensor with internal signal conditioning block (ADC)